## IN0

1. Gnd GREEN
2. +5 regulated ORANGE
3. Input signal BLUE

## IN1

1. Gnd
2. +5 regulated
3. Input signal

## IN2 (bridge sensor amplifier included)

1. -5 regulated
2. +5 regulated
3. Input signal +
4. Input signal –

## OPTO

1. Opt0-1
2. Opto-1
3. Opto-0
4. Opto-0

## Power

1. Gnd
2. Unregulated +9V
3. Unregulated -9V

## RAW

1. Gnd GREEN
2. Raw 0 BLUE
3. Raw 1 BROWN